**Required Materials**

1. Slim Wood (100\*100 cm)
2. Wood (200\*200 cm)
3. Wood Adhesive
4. Strings of Instrument
5. Nail
6. Screw

**Step 1**

Wood is cut for base and lateral surfaces.

**Step 2**



Interrupted surfaces are nailed

**Step 3 (Make Upper)**

Mixed Guitar’s upper is cut and it’s holes are opened.

**Step 4**




Upper is nailed to the box which had made before.

**Step 5 (Make Bridge)**

The lower bridge is holed to pass the strings and nailed to the side of the box.

**Step 6 (Make Pegbox)**



Roller stick is cut each 4 cm, inside of them are carved.

Pegboxes are holed to pass the string

**Step 8**

Strings are attached on the bridge by streching.